Transducer - Array


US-Windows = < 3mm Epoxy


Ground





          Cork / Neopren




Piezo – 1







Piezo – 2





Copper shield





Neopren  1mm

 shielded enclosure Alu


cavity fill with PU

Electric connections


Wire-bridge

Ground




Piezo – 1







Piezo - 2
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